MyPAM Connections required

Motor Driver boards: direction (DIO0, pin 11), PWM (DIO8/PWM0/pin 27), GND (pin 30)

Encoders:

Potentiometers





